(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "CH340N" (in_bom yes) (on_board yes)
    (property "Reference" "U3" (at 1.9559 -1.27 0))
    (property "Value" "CH340N" (at -8.89 -1.27 0))
    (property "Footprint" "Package_SO:SOP-8_3.9x4.9mm_P1.27mm" (at 1.27 -13.97 0))
    (property "Datasheet" "https://datasheet.lcsc.com/szlcsc/Jiangsu-Qin-Heng-CH340C_C84681.pdf" (at -8.89 20.32 0))
    (property "LCSC" "C2977777" (at 0 0 0))
    (property "ki_keywords" "USB UART Serial Converter Interface" (at 0 0 0))
    (property "ki_description" "USB serial converter, UART, SOP-8" (at 0 0 0))
    (property "ki_fp_filters" "SOP*3.9x4.9mm*P1.27mm*" (at 0 0 0))
    (symbol "CH340N_0_1")
    (symbol "CH340N_1_1"
      (pin bidirectional line (at -10.16 7.62 0) (length 2.54)
        (name "UD+")
        (number "1")
      )
      (pin bidirectional line (at -10.16 5.08 0) (length 2.54)
        (name "UD-")
        (number "2")
      )
      (pin power_in line (at 0 -1.27 90) (length 2.54)
        (name "GND")
        (number "3")
      )
      (pin output line (at 10.16 3.81 180) (length 2.54)
        (name "~{RTS}")
        (number "4")
      )
      (pin power_in line (at 0 15.24 270) (length 2.54)
        (name "VCC")
        (number "5")
      )
      (pin output line (at 10.16 10.16 180) (length 2.54)
        (name "TXD")
        (number "6")
      )
      (pin input line (at 10.16 7.62 180) (length 2.54)
        (name "RXD")
        (number "7")
      )
      (pin passive line (at -2.54 15.24 270) (length 2.54)
        (name "V3")
        (number "8")
      )
    )
  )
)
